From 1b39a1834ed182bbd8036a5cd74a9ea111fa4691 Mon Sep 17 00:00:00 2001
From: Andre Przywara <andre.przywara@arm.com>
Date: Mon, 29 Oct 2018 00:56:47 +0000
Subject: [PATCH 03/13] sunxi: A64: Update .dts/.dtsi files
MIME-Version: 1.0
Content-Type: text/plain; charset=UTF-8
Content-Transfer-Encoding: 8bit

Update the .dts/.dtsi file from the Linux sunxi/dt64-for-4.20 tree:
commit 679294497be31596e1c9c61507746d72b6b05f26
Author: Rodrigo Exterckötter Tjäder <rodrigo@tjader.xyz>
Date:   Wed Sep 26 19:48:24 2018 +0000
    arm64: dts: allwinner: a64: a64-olinuxino: set the PHY TX delay

Signed-off-by: Andre Przywara <andre.przywara@arm.com>
Acked-by: Maxime Ripard <maxime.ripard@bootlin.com>
Reviewed-by: Jagan Teki <jagan@openedev.com>
---
 arch/arm/dts/sun50i-a64-amarula-relic.dts    | 168 +++++++++++++-
 arch/arm/dts/sun50i-a64-bananapi-m64.dts     |  34 ++-
 arch/arm/dts/sun50i-a64-nanopi-a64.dts       |  89 +++++++-
 arch/arm/dts/sun50i-a64-olinuxino.dts        | 103 ++++++++-
 arch/arm/dts/sun50i-a64-orangepi-win.dts     | 179 ++++++++++++++-
 arch/arm/dts/sun50i-a64-pine64.dts           |  32 ++-
 arch/arm/dts/sun50i-a64-sopine-baseboard.dts |  32 ++-
 arch/arm/dts/sun50i-a64-sopine.dtsi          |  15 ++
 arch/arm/dts/sun50i-a64.dtsi                 | 313 +++++++++++++++++++++++++--
 9 files changed, 920 insertions(+), 45 deletions(-)

diff --git a/arch/arm/dts/sun50i-a64-amarula-relic.dts b/arch/arm/dts/sun50i-a64-amarula-relic.dts
index f3b4e93ece..6cb2b7f0c8 100644
--- a/arch/arm/dts/sun50i-a64-amarula-relic.dts
+++ b/arch/arm/dts/sun50i-a64-amarula-relic.dts
@@ -22,11 +22,11 @@
 		stdout-path = "serial0:115200n8";
 	};
 
-	reg_vcc3v3: vcc3v3 {
-		compatible = "regulator-fixed";
-		regulator-name = "vcc3v3";
-		regulator-min-microvolt = <3300000>;
-		regulator-max-microvolt = <3300000>;
+	wifi_pwrseq: wifi-pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* WL-PMU-EN: PL2 */
 	};
 };
 
@@ -34,10 +34,34 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dcdc1>;
+	/*
+	 * Schematic shows both dldo4 and eldo1 connected for vcc-io-wifi, but
+	 * dldo4 connection shows DNP(Do Not Populate) and eldo1 connected with
+	 * 0Ohm register to vcc-io-wifi so eldo1 is used.
+	 */
+	vqmmc-supply = <&reg_eldo1>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>;	/* WL-WAKE-AP: PL3 */
+		interrupt-names = "host-wake";
+	};
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_pins>;
-	vmmc-supply = <&reg_vcc3v3>;
+	vmmc-supply = <&reg_dcdc1>;
 	bus-width = <8>;
 	non-removable;
 	cap-mmc-hw-reset;
@@ -48,9 +72,138 @@
 	status = "okay";
 };
 
+&r_rsb {
+	status = "okay";
+
+	axp803: pmic@3a3 {
+		compatible = "x-powers,axp803";
+		reg = <0x3a3>;
+		interrupt-parent = <&r_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		x-powers,drive-vbus-en; /* set N_VBUSEN as output pin */
+	};
+};
+
+#include "axp803.dtsi"
+
+&reg_aldo1 {
+	regulator-always-on;
+	regulator-min-microvolt = <2800000>;
+	regulator-max-microvolt = <2800000>;
+	regulator-name = "avdd-csi";
+};
+
+&reg_aldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-pl";
+};
+
+&reg_aldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <3000000>;
+	regulator-max-microvolt = <3000000>;
+	regulator-name = "vcc-pll-avcc";
+};
+
+&reg_dcdc1 {
+	regulator-always-on;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-3v3";
+};
+
+&reg_dcdc2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1040000>;
+	regulator-max-microvolt = <1300000>;
+	regulator-name = "vdd-cpux";
+};
+
+/* DCDC3 is polyphased with DCDC2 */
+
+&reg_dcdc5 {
+	regulator-always-on;
+	regulator-min-microvolt = <1500000>;
+	regulator-max-microvolt = <1500000>;
+	regulator-name = "vcc-dram";
+};
+
+&reg_dcdc6 {
+	regulator-always-on;
+	regulator-min-microvolt = <1100000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-sys";
+};
+
+&reg_dldo1 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-hdmi-dsi-sensor";
+};
+
+&reg_dldo2 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-mipi";
+};
+
+&reg_dldo3 {
+	regulator-min-microvolt = <2800000>;
+	regulator-max-microvolt = <2800000>;
+	regulator-name = "dovdd-csi";
+};
+
+&reg_dldo4 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-wifi-io";
+};
+
+&reg_drivevbus {
+	regulator-name = "usb0-vbus";
+	status = "okay";
+};
+
+&reg_eldo1 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "cpvdd";
+};
+
+&reg_eldo3 {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "dvdd-csi";
+};
+
+&reg_fldo1 {
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "vcc-1v2-hsic";
+};
+
+/*
+ * The A64 chip cannot work without this regulator off, although
+ * it seems to be only driving the AR100 core.
+ * Maybe we don't still know well about CPUs domain.
+ */
+&reg_fldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1100000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpus";
+};
+
+&reg_rtc_ldo {
+	regulator-name = "vcc-rtc";
+};
+
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
@@ -61,5 +214,6 @@
 
 &usbphy {
 	usb0_id_det-gpios = <&pio 7 9 GPIO_ACTIVE_HIGH>; /* PH9 */
+	usb0_vbus-supply = <&reg_drivevbus>;
 	status = "okay";
 };
diff --git a/arch/arm/dts/sun50i-a64-bananapi-m64.dts b/arch/arm/dts/sun50i-a64-bananapi-m64.dts
index 0716b14411..ef1c90401b 100644
--- a/arch/arm/dts/sun50i-a64-bananapi-m64.dts
+++ b/arch/arm/dts/sun50i-a64-bananapi-m64.dts
@@ -60,6 +60,17 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -86,6 +97,10 @@
 	};
 };
 
+&de {
+	status = "okay";
+};
+
 &ehci0 {
 	status = "okay";
 };
@@ -103,6 +118,17 @@
 	status = "okay";
 };
 
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &i2c1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c1_pins>;
@@ -151,7 +177,7 @@
 
 &mmc2 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&mmc2_pins>;
+	pinctrl-0 = <&mmc2_pins>, <&mmc2_ds_pin>;
 	vmmc-supply = <&reg_dcdc1>;
 	bus-width = <8>;
 	non-removable;
@@ -296,9 +322,13 @@
 	regulator-name = "vcc-rtc";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
diff --git a/arch/arm/dts/sun50i-a64-nanopi-a64.dts b/arch/arm/dts/sun50i-a64-nanopi-a64.dts
index e2dce48fa2..31884dbc88 100644
--- a/arch/arm/dts/sun50i-a64-nanopi-a64.dts
+++ b/arch/arm/dts/sun50i-a64-nanopi-a64.dts
@@ -51,12 +51,44 @@
 	compatible = "friendlyarm,nanopi-a64", "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		blue {
+			label = "nanopi-a64:blue:status";
+			gpios = <&pio 3 24 GPIO_ACTIVE_LOW>; /* PD24 */
+		};
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
+	};
+};
+
+&de {
+	status = "okay";
 };
 
 &ehci0 {
@@ -67,6 +99,26 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_dcdc1>;
+	status = "okay";
+};
+
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 /* i2c1 connected with gpio headers like pine64, bananapi */
 &i2c1 {
 	pinctrl-names = "default";
@@ -78,6 +130,13 @@
 	bias-pull-up;
 };
 
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
@@ -88,6 +147,24 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dcdc1>;
+	vqmmc-supply = <&reg_dldo4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	rtl8189etv: wifi@1 {
+		reg = <1>;
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>; /* PL3 */
+		interrupt-names = "host-wake";
+	};
+};
+
 &ohci0 {
 	status = "okay";
 };
@@ -125,9 +202,9 @@
 
 &reg_dcdc1 {
 	regulator-always-on;
-	regulator-min-microvolt = <3000000>;
-	regulator-max-microvolt = <3000000>;
-	regulator-name = "vcc-3v";
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-3v3";
 };
 
 &reg_dcdc2 {
@@ -195,9 +272,13 @@
 	regulator-name = "vcc-rtc";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
diff --git a/arch/arm/dts/sun50i-a64-olinuxino.dts b/arch/arm/dts/sun50i-a64-olinuxino.dts
index 3b3081b10e..f7a4bccaa5 100644
--- a/arch/arm/dts/sun50i-a64-olinuxino.dts
+++ b/arch/arm/dts/sun50i-a64-olinuxino.dts
@@ -51,6 +51,7 @@
 	compatible = "olimex,a64-olinuxino", "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -58,12 +59,74 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	reg_usb1_vbus: usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 6 9 GPIO_ACTIVE_HIGH>; /* PG9 */
+		status = "okay";
+	};
+
 	wifi_pwrseq: wifi_pwrseq {
 		compatible = "mmc-pwrseq-simple";
 		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
 	};
 };
 
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_dcdc1>;
+	allwinner,tx-delay-ps = <600>;
+	status = "okay";
+};
+
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
@@ -92,6 +155,14 @@
 	};
 };
 
+&ohci0 {
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
 &r_rsb {
 	status = "okay";
 
@@ -100,6 +171,7 @@
 		reg = <0x3a3>;
 		interrupt-parent = <&r_intc>;
 		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		x-powers,drive-vbus-en;	/* set N_VBUSEN as output pin */
 	};
 };
 
@@ -142,10 +214,14 @@
 
 /* DCDC3 is polyphased with DCDC2 */
 
+/*
+ * The board uses DDR3L DRAM chips. 1.36V is the closest to the nominal
+ * 1.35V that the PMIC can drive.
+ */
 &reg_dcdc5 {
 	regulator-always-on;
-	regulator-min-microvolt = <1500000>;
-	regulator-max-microvolt = <1500000>;
+	regulator-min-microvolt = <1360000>;
+	regulator-max-microvolt = <1360000>;
 	regulator-name = "vcc-ddr3";
 };
 
@@ -180,6 +256,11 @@
 	regulator-name = "vcc-wifi-io";
 };
 
+&reg_drivevbus {
+	regulator-name = "usb0-vbus";
+	status = "okay";
+};
+
 &reg_eldo1 {
 	regulator-min-microvolt = <1800000>;
 	regulator-max-microvolt = <1800000>;
@@ -214,8 +295,24 @@
 	regulator-name = "vcc-rtc";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
 	status = "okay";
+	usb0_id_det-gpios = <&pio 7 9 GPIO_ACTIVE_HIGH>; /* PH9 */
+	usb0_vbus-supply = <&reg_drivevbus>;
+	usb1_vbus-supply = <&reg_usb1_vbus>;
 };
diff --git a/arch/arm/dts/sun50i-a64-orangepi-win.dts b/arch/arm/dts/sun50i-a64-orangepi-win.dts
index bf42690a33..b0c64f7579 100644
--- a/arch/arm/dts/sun50i-a64-orangepi-win.dts
+++ b/arch/arm/dts/sun50i-a64-orangepi-win.dts
@@ -1,5 +1,6 @@
 /*
  * Copyright (C) 2017 Jagan Teki <jteki@openedev.com>
+ * Copyright (C) 2017-2018 Samuel Holland <samuel@sholland.org>
  *
  * This file is dual-licensed: you can use it either under the terms
  * of the GPL or the X11 license, at your option. Note that this dual
@@ -51,23 +52,127 @@
 	compatible = "xunlong,orangepi-win", "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
+		serial1 = &uart1;
+		serial2 = &uart2;
+		serial3 = &uart3;
+		serial4 = &uart4;
 	};
 
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		status {
+			label = "orangepi:green:status";
+			gpios = <&pio 7 11 GPIO_ACTIVE_HIGH>; /* PH11 */
+		};
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 14 GPIO_ACTIVE_HIGH>; /* PD14 */
+		status = "okay";
+	};
+
+	reg_usb1_vbus: usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 7 GPIO_ACTIVE_HIGH>; /* PD7 */
+		status = "okay";
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 8 GPIO_ACTIVE_LOW>; /* PL8 */
+	};
+};
+
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
 };
 
 &ehci1 {
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_gmac_3v3>;
+	status = "okay";
+};
+
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
 	vmmc-supply = <&reg_dcdc1>;
-	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
+	disable-wp;
+	bus-width = <4>;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dldo2>;
+	vqmmc-supply = <&reg_dldo4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+};
+
+&ohci0 {
 	status = "okay";
 };
 
@@ -89,9 +194,8 @@
 #include "axp803.dtsi"
 
 &reg_aldo1 {
-	regulator-always-on;
-	regulator-min-microvolt = <1800000>;
-	regulator-max-microvolt = <3300000>;
+	regulator-min-microvolt = <2800000>;
+	regulator-max-microvolt = <2800000>;
 	regulator-name = "afvcc-csi";
 };
 
@@ -163,12 +267,23 @@
 	regulator-name = "vcc-wifi-io";
 };
 
+&reg_drivevbus {
+	regulator-name = "usb0-vbus";
+	status = "okay";
+};
+
 &reg_eldo1 {
 	regulator-min-microvolt = <1800000>;
 	regulator-max-microvolt = <1800000>;
 	regulator-name = "cpvdd";
 };
 
+&reg_eldo3 {
+	regulator-min-microvolt = <1500000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "dvdd-csi";
+};
+
 &reg_fldo1 {
 	regulator-min-microvolt = <1200000>;
 	regulator-max-microvolt = <1200000>;
@@ -191,13 +306,65 @@
 	regulator-name = "vcc-rtc";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
+&spi0 {
+	status = "okay";
+
+	spi-flash@0 {
+		compatible = "mxicy,mx25l1606e", "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <80000000>;
+		m25p,fast-read;
+		status = "okay";
+	};
+};
+
+/* On debug connector */
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
-&usbphy {
+/* Bluetooth */
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
+	status = "okay";
+};
+
+/* On Pi-2 connector, RTS/CTS optional */
+&uart2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart2_pins>;
+	status = "disabled";
+};
+
+/* On Pi-2 connector, RTS/CTS optional */
+&uart3 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart3_pins>;
+	status = "disabled";
+};
+
+/* On Pi-2 connector (labeled for SPI1), RTS/CTS optional */
+&uart4 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart4_pins>;
+	status = "disabled";
+};
+
+&usb_otg {
+	dr_mode = "otg";
 	status = "okay";
 };
 
+&usbphy {
+	usb0_id_det-gpios = <&pio 7 9 GPIO_ACTIVE_HIGH>; /* PH9 */
+	usb0_vbus-supply = <&reg_drivevbus>;
+	usb1_vbus-supply = <&reg_usb1_vbus>;
+	status = "okay";
+};
diff --git a/arch/arm/dts/sun50i-a64-pine64.dts b/arch/arm/dts/sun50i-a64-pine64.dts
index a75825798a..c077b6c1f4 100644
--- a/arch/arm/dts/sun50i-a64-pine64.dts
+++ b/arch/arm/dts/sun50i-a64-pine64.dts
@@ -62,6 +62,21 @@
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+};
+
+&de {
+	status = "okay";
 };
 
 &ehci0 {
@@ -82,6 +97,17 @@
 
 };
 
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &i2c1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c1_pins>;
@@ -229,6 +255,10 @@
 	regulator-name = "vcc-rtc";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
 /* On Euler connector */
 &spdif {
 	status = "disabled";
@@ -237,7 +267,7 @@
 /* On Exp and Euler connectors */
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
diff --git a/arch/arm/dts/sun50i-a64-sopine-baseboard.dts b/arch/arm/dts/sun50i-a64-sopine-baseboard.dts
index abe179de35..53fcc9098d 100644
--- a/arch/arm/dts/sun50i-a64-sopine-baseboard.dts
+++ b/arch/arm/dts/sun50i-a64-sopine-baseboard.dts
@@ -61,6 +61,17 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	hdmi-connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	reg_vcc1v8: vcc1v8 {
 		compatible = "regulator-fixed";
 		regulator-name = "vcc1v8";
@@ -69,6 +80,10 @@
 	};
 };
 
+&de {
+	status = "okay";
+};
+
 &ehci0 {
 	status = "okay";
 };
@@ -86,6 +101,17 @@
 	status = "okay";
 };
 
+&hdmi {
+	hvcc-supply = <&reg_dldo1>;
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
 &mdio {
 	ext_rgmii_phy: ethernet-phy@1 {
 		compatible = "ethernet-phy-ieee802.3-c22";
@@ -134,9 +160,13 @@
 	regulator-name = "vcc-wifi";
 };
 
+&simplefb_hdmi {
+	vcc-hdmi-supply = <&reg_dldo1>;
+};
+
 &uart0 {
 	pinctrl-names = "default";
-	pinctrl-0 = <&uart0_pins_a>;
+	pinctrl-0 = <&uart0_pb_pins>;
 	status = "okay";
 };
 
diff --git a/arch/arm/dts/sun50i-a64-sopine.dtsi b/arch/arm/dts/sun50i-a64-sopine.dtsi
index 43418bd881..6723b8695e 100644
--- a/arch/arm/dts/sun50i-a64-sopine.dtsi
+++ b/arch/arm/dts/sun50i-a64-sopine.dtsi
@@ -45,6 +45,8 @@
 
 #include "sun50i-a64.dtsi"
 
+#include <dt-bindings/gpio/gpio.h>
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
@@ -52,6 +54,7 @@
 	non-removable;
 	disable-wp;
 	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
 	status = "okay";
 };
 
@@ -66,6 +69,18 @@
 	};
 };
 
+&spi0  {
+	status = "okay";
+
+	flash@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "jedec,spi-nor";
+		reg = <0>;
+		spi-max-frequency = <40000000>;
+	};
+};
+
 #include "axp803.dtsi"
 
 &reg_aldo2 {
diff --git a/arch/arm/dts/sun50i-a64.dtsi b/arch/arm/dts/sun50i-a64.dtsi
index 7a083637c4..f3a66f8882 100644
--- a/arch/arm/dts/sun50i-a64.dtsi
+++ b/arch/arm/dts/sun50i-a64.dtsi
@@ -43,9 +43,12 @@
  */
 
 #include <dt-bindings/clock/sun50i-a64-ccu.h>
+#include <dt-bindings/clock/sun8i-de2.h>
 #include <dt-bindings/clock/sun8i-r-ccu.h>
 #include <dt-bindings/interrupt-controller/arm-gic.h>
 #include <dt-bindings/reset/sun50i-a64-ccu.h>
+#include <dt-bindings/reset/sun8i-de2.h>
+#include <dt-bindings/reset/sun8i-r-ccu.h>
 
 / {
 	interrupt-parent = <&gic>;
@@ -57,17 +60,21 @@
 		#size-cells = <1>;
 		ranges;
 
-/*
- * The pipeline mixer0-lcd0 depends on clock CLK_MIXER0 from DE2 CCU.
- * However there is no support for this clock on A64 yet, so we depend
- * on the upstream clocks here to keep them (and thus CLK_MIXER0) up.
- */
 		simplefb_lcd: framebuffer-lcd {
 			compatible = "allwinner,simple-framebuffer",
 				     "simple-framebuffer";
 			allwinner,pipeline = "mixer0-lcd0";
 			clocks = <&ccu CLK_TCON0>,
-				 <&ccu CLK_DE>, <&ccu CLK_BUS_DE>;
+				 <&display_clocks CLK_MIXER0>;
+			status = "disabled";
+		};
+
+		simplefb_hdmi: framebuffer-hdmi {
+			compatible = "allwinner,simple-framebuffer",
+				     "simple-framebuffer";
+			allwinner,pipeline = "mixer1-lcd1-hdmi";
+			clocks = <&display_clocks CLK_MIXER1>,
+				 <&ccu CLK_TCON1>, <&ccu CLK_HDMI>;
 			status = "disabled";
 		};
 	};
@@ -81,6 +88,7 @@
 			device_type = "cpu";
 			reg = <0>;
 			enable-method = "psci";
+			next-level-cache = <&L2>;
 		};
 
 		cpu1: cpu@1 {
@@ -88,6 +96,7 @@
 			device_type = "cpu";
 			reg = <1>;
 			enable-method = "psci";
+			next-level-cache = <&L2>;
 		};
 
 		cpu2: cpu@2 {
@@ -95,6 +104,7 @@
 			device_type = "cpu";
 			reg = <2>;
 			enable-method = "psci";
+			next-level-cache = <&L2>;
 		};
 
 		cpu3: cpu@3 {
@@ -102,7 +112,20 @@
 			device_type = "cpu";
 			reg = <3>;
 			enable-method = "psci";
+			next-level-cache = <&L2>;
 		};
+
+		L2: l2-cache {
+			compatible = "cache";
+			cache-level = <2>;
+		};
+	};
+
+	de: display-engine {
+		compatible = "allwinner,sun50i-a64-display-engine";
+		allwinner,pipelines = <&mixer0>,
+				      <&mixer1>;
+		status = "disabled";
 	};
 
 	osc24M: osc24M_clk {
@@ -168,10 +191,92 @@
 		#size-cells = <1>;
 		ranges;
 
+		de2@1000000 {
+			compatible = "allwinner,sun50i-a64-de2";
+			reg = <0x1000000 0x400000>;
+			allwinner,sram = <&de2_sram 1>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges = <0 0x1000000 0x400000>;
+
+			display_clocks: clock@0 {
+				compatible = "allwinner,sun50i-a64-de2-clk";
+				reg = <0x0 0x100000>;
+				clocks = <&ccu CLK_DE>,
+					 <&ccu CLK_BUS_DE>;
+				clock-names = "mod",
+					      "bus";
+				resets = <&ccu RST_BUS_DE>;
+				#clock-cells = <1>;
+				#reset-cells = <1>;
+			};
+
+			mixer0: mixer@100000 {
+				compatible = "allwinner,sun50i-a64-de2-mixer-0";
+				reg = <0x100000 0x100000>;
+				clocks = <&display_clocks CLK_BUS_MIXER0>,
+					 <&display_clocks CLK_MIXER0>;
+				clock-names = "bus",
+					      "mod";
+				resets = <&display_clocks RST_MIXER0>;
+
+				ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					mixer0_out: port@1 {
+						reg = <1>;
+
+						mixer0_out_tcon0: endpoint {
+							remote-endpoint = <&tcon0_in_mixer0>;
+						};
+					};
+				};
+			};
+
+			mixer1: mixer@200000 {
+				compatible = "allwinner,sun50i-a64-de2-mixer-1";
+				reg = <0x200000 0x100000>;
+				clocks = <&display_clocks CLK_BUS_MIXER1>,
+					 <&display_clocks CLK_MIXER1>;
+				clock-names = "bus",
+					      "mod";
+				resets = <&display_clocks RST_MIXER1>;
+
+				ports {
+					#address-cells = <1>;
+					#size-cells = <0>;
+
+					mixer1_out: port@1 {
+						reg = <1>;
+
+						mixer1_out_tcon1: endpoint {
+							remote-endpoint = <&tcon1_in_mixer1>;
+						};
+					};
+				};
+			};
+		};
+
 		syscon: syscon@1c00000 {
-			compatible = "allwinner,sun50i-a64-system-controller",
-				"syscon";
+			compatible = "allwinner,sun50i-a64-system-control";
 			reg = <0x01c00000 0x1000>;
+			#address-cells = <1>;
+			#size-cells = <1>;
+			ranges;
+
+			sram_c: sram@18000 {
+				compatible = "mmio-sram";
+				reg = <0x00018000 0x28000>;
+				#address-cells = <1>;
+				#size-cells = <1>;
+				ranges = <0 0x00018000 0x28000>;
+
+				de2_sram: sram-section@0 {
+					compatible = "allwinner,sun50i-a64-sram-c";
+					reg = <0x0000 0x28000>;
+				};
+			};
 		};
 
 		dma: dma-controller@1c02000 {
@@ -185,6 +290,75 @@
 			#dma-cells = <1>;
 		};
 
+		tcon0: lcd-controller@1c0c000 {
+			compatible = "allwinner,sun50i-a64-tcon-lcd",
+				     "allwinner,sun8i-a83t-tcon-lcd";
+			reg = <0x01c0c000 0x1000>;
+			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON0>, <&ccu CLK_TCON0>;
+			clock-names = "ahb", "tcon-ch0";
+			clock-output-names = "tcon-pixel-clock";
+			resets = <&ccu RST_BUS_TCON0>, <&ccu RST_BUS_LVDS>;
+			reset-names = "lcd", "lvds";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon0_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					tcon0_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon0>;
+					};
+				};
+
+				tcon0_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+			};
+		};
+
+		tcon1: lcd-controller@1c0d000 {
+			compatible = "allwinner,sun50i-a64-tcon-tv",
+				     "allwinner,sun8i-a83t-tcon-tv";
+			reg = <0x01c0d000 0x1000>;
+			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON1>, <&ccu CLK_TCON1>;
+			clock-names = "ahb", "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON1>;
+			reset-names = "lcd";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon1_in: port@0 {
+					reg = <0>;
+
+					tcon1_in_mixer1: endpoint {
+						remote-endpoint = <&mixer1_out_tcon1>;
+					};
+				};
+
+				tcon1_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					tcon1_out_hdmi: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&hdmi_in_tcon1>;
+					};
+				};
+			};
+		};
+
 		mmc0: mmc@1c0f000 {
 			compatible = "allwinner,sun50i-a64-mmc";
 			reg = <0x01c0f000 0x1000>;
@@ -227,6 +401,11 @@
 			#size-cells = <0>;
 		};
 
+		sid: eeprom@1c14000 {
+			compatible = "allwinner,sun50i-a64-sid";
+			reg = <0x1c14000 0x400>;
+		};
+
 		usb_otg: usb@1c19000 {
 			compatible = "allwinner,sun8i-a33-musb";
 			reg = <0x01c19000 0x0400>;
@@ -356,7 +535,7 @@
 			};
 
 			mmc2_pins: mmc2-pins {
-				pins = "PC1", "PC5", "PC6", "PC8", "PC9",
+				pins = "PC5", "PC6", "PC8", "PC9",
 				       "PC10","PC11", "PC12", "PC13",
 				       "PC14", "PC15", "PC16";
 				function = "mmc2";
@@ -364,6 +543,18 @@
 				bias-pull-up;
 			};
 
+			mmc2_ds_pin: mmc2-ds-pin {
+				pins = "PC1";
+				function = "mmc2";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
+			pwm_pin: pwm_pin {
+				pins = "PD22";
+				function = "pwm";
+			};
+
 			rmii_pins: rmii_pins {
 				pins = "PD10", "PD11", "PD13", "PD14", "PD17",
 				       "PD18", "PD19", "PD20", "PD22", "PD23";
@@ -394,7 +585,7 @@
 				function = "spi1";
 			};
 
-			uart0_pins_a: uart0 {
+			uart0_pb_pins: uart0-pb-pins {
 				pins = "PB8", "PB9";
 				function = "uart0";
 			};
@@ -474,15 +665,6 @@
 			status = "disabled";
 		};
 
-		pwm: pwm@1c21400 {
-			compatible = "allwinner,sun50i-a64-pwm",
-				     "allwinner,sun5i-a13-pwm";
-			reg = <0x01c21400 0x8>;
-			clocks = <&osc24M>;
-			#pwm-cells = <3>;
-			status = "disabled";
-		};
-
 		uart0: serial@1c28000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28000 0x400>;
@@ -617,8 +799,6 @@
 			clocks = <&ccu CLK_BUS_EMAC>;
 			clock-names = "stmmaceth";
 			status = "disabled";
-			#address-cells = <1>;
-			#size-cells = <0>;
 
 			mdio: mdio {
 				compatible = "snps,dwmac-mdio";
@@ -638,11 +818,69 @@
 			#interrupt-cells = <3>;
 		};
 
+		pwm: pwm@1c21400 {
+			compatible = "allwinner,sun50i-a64-pwm",
+				     "allwinner,sun5i-a13-pwm";
+			reg = <0x01c21400 0x400>;
+			clocks = <&osc24M>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&pwm_pin>;
+			#pwm-cells = <3>;
+			status = "disabled";
+		};
+
+		hdmi: hdmi@1ee0000 {
+			compatible = "allwinner,sun50i-a64-dw-hdmi",
+				     "allwinner,sun8i-a83t-dw-hdmi";
+			reg = <0x01ee0000 0x10000>;
+			reg-io-width = <1>;
+			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_DDC>,
+				 <&ccu CLK_HDMI>;
+			clock-names = "iahb", "isfr", "tmds";
+			resets = <&ccu RST_BUS_HDMI1>;
+			reset-names = "ctrl";
+			phys = <&hdmi_phy>;
+			phy-names = "hdmi-phy";
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				hdmi_in: port@0 {
+					reg = <0>;
+
+					hdmi_in_tcon1: endpoint {
+						remote-endpoint = <&tcon1_out_hdmi>;
+					};
+				};
+
+				hdmi_out: port@1 {
+					reg = <1>;
+				};
+			};
+		};
+
+		hdmi_phy: hdmi-phy@1ef0000 {
+			compatible = "allwinner,sun50i-a64-hdmi-phy";
+			reg = <0x01ef0000 0x10000>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_DDC>,
+				 <&ccu 7>;
+			clock-names = "bus", "mod", "pll-0";
+			resets = <&ccu RST_BUS_HDMI0>;
+			reset-names = "phy";
+			#phy-cells = <0>;
+		};
+
 		rtc: rtc@1f00000 {
 			compatible = "allwinner,sun6i-a31-rtc";
 			reg = <0x01f00000 0x54>;
 			interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>,
 				     <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
+			clock-output-names = "rtc-osc32k", "rtc-osc32k-out";
+			clocks = <&osc32k>;
+			#clock-cells = <1>;
 		};
 
 		r_intc: interrupt-controller@1f00c00 {
@@ -664,6 +902,29 @@
 			#reset-cells = <1>;
 		};
 
+		r_i2c: i2c@1f02400 {
+			compatible = "allwinner,sun50i-a64-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x01f02400 0x400>;
+			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&r_ccu CLK_APB0_I2C>;
+			resets = <&r_ccu RST_APB0_I2C>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		r_pwm: pwm@1f03800 {
+			compatible = "allwinner,sun50i-a64-pwm",
+				     "allwinner,sun5i-a13-pwm";
+			reg = <0x01f03800 0x400>;
+			clocks = <&osc24M>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&r_pwm_pin>;
+			#pwm-cells = <3>;
+			status = "disabled";
+		};
+
 		r_pio: pinctrl@1f02c00 {
 			compatible = "allwinner,sun50i-a64-r-pinctrl";
 			reg = <0x01f02c00 0x400>;
@@ -675,6 +936,16 @@
 			interrupt-controller;
 			#interrupt-cells = <3>;
 
+			r_i2c_pl89_pins: r-i2c-pl89-pins {
+				pins = "PL8", "PL9";
+				function = "s_i2c";
+			};
+
+			r_pwm_pin: pwm {
+				pins = "PL10";
+				function = "s_pwm";
+			};
+
 			r_rsb_pins: rsb {
 				pins = "PL0", "PL1";
 				function = "s_rsb";
-- 
2.11.0

