From a88a3f887181605f4487a22bdfb7d87ffafde5d9 Mon Sep 17 00:00:00 2001
From: Jan Beulich <jbeulich@suse.com>
Date: Tue, 2 Jun 2015 15:07:01 +0000
Subject: [PATCH] xen/pt: add a few PCI config space field descriptions

Since the next patch will turn all not explicitly described fields
read-only by default, those fields that have guest writable bits need
to be given explicit descriptors.

This is a preparatory patch for XSA-131.

Signed-off-by: Jan Beulich <jbeulich@suse.com>
---
 hw/xen/xen_pt_config_init.c | 28 ++++++++++++++++++++++++++++
 1 file changed, 28 insertions(+)

diff --git a/hw/xen/xen_pt_config_init.c b/hw/xen/xen_pt_config_init.c
index efd8bac..19f926b 100644
--- a/hw/xen/xen_pt_config_init.c
+++ b/hw/xen/xen_pt_config_init.c
@@ -754,6 +754,15 @@ static XenPTRegInfo xen_pt_emu_reg_vpd[] = {
         .u.b.write  = xen_pt_byte_reg_write,
     },
     {
+        .offset     = PCI_VPD_ADDR,
+        .size       = 2,
+        .ro_mask    = 0x0003,
+        .emu_mask   = 0x0003,
+        .init       = xen_pt_common_reg_init,
+        .u.w.read   = xen_pt_word_reg_read,
+        .u.w.write  = xen_pt_word_reg_write,
+    },
+    {
         .size = 0,
     },
 };
@@ -889,6 +898,16 @@ static XenPTRegInfo xen_pt_emu_reg_pcie[] = {
         .u.w.read   = xen_pt_word_reg_read,
         .u.w.write  = xen_pt_word_reg_write,
     },
+    /* Device Status reg */
+    {
+        .offset     = PCI_EXP_DEVSTA,
+        .size       = 2,
+        .res_mask   = 0xFFC0,
+        .ro_mask    = 0x0030,
+        .init       = xen_pt_common_reg_init,
+        .u.w.read   = xen_pt_word_reg_read,
+        .u.w.write  = xen_pt_word_reg_write,
+    },
     /* Link Control reg */
     {
         .offset     = PCI_EXP_LNKCTL,
@@ -900,6 +919,15 @@ static XenPTRegInfo xen_pt_emu_reg_pcie[] = {
         .u.w.read   = xen_pt_word_reg_read,
         .u.w.write  = xen_pt_word_reg_write,
     },
+    /* Link Status reg */
+    {
+        .offset     = PCI_EXP_LNKSTA,
+        .size       = 2,
+        .ro_mask    = 0x3FFF,
+        .init       = xen_pt_common_reg_init,
+        .u.w.read   = xen_pt_word_reg_read,
+        .u.w.write  = xen_pt_word_reg_write,
+    },
     /* Device Control 2 reg */
     {
         .offset     = 0x28,
-- 
2.2.1

