From 7611dae8a69f0f1775ba1a9a942961c2aa10d88e Mon Sep 17 00:00:00 2001
From: Jan Beulich <jbeulich@suse.com>
Date: Tue, 2 Jun 2015 15:07:00 +0000
Subject: [PATCH] xen: don't allow guest to control MSI mask register

It's being used by the hypervisor. For now simply mimic a device not
capable of masking, and fully emulate any accesses a guest may issue
nevertheless as simple reads/writes without side effects.

This is XSA-129.

Signed-off-by: Jan Beulich <jbeulich@suse.com>
Reviewed-by: Stefano Stabellini <stefano.stabellini@eu.citrix.com>
---
 hw/pci/msi.c                |  4 --
 hw/xen/xen_pt_config_init.c | 98 ++++++++++++++++++++++++++++++++++++++++-----
 include/hw/pci/pci_regs.h   |  2 +
 3 files changed, 90 insertions(+), 14 deletions(-)

diff --git a/hw/pci/msi.c b/hw/pci/msi.c
index c111dba..f9c0484 100644
--- a/hw/pci/msi.c
+++ b/hw/pci/msi.c
@@ -21,10 +21,6 @@
 #include "hw/pci/msi.h"
 #include "qemu/range.h"
 
-/* Eventually those constants should go to Linux pci_regs.h */
-#define PCI_MSI_PENDING_32      0x10
-#define PCI_MSI_PENDING_64      0x14
-
 /* PCI_MSI_ADDRESS_LO */
 #define PCI_MSI_ADDRESS_LO_MASK         (~0x3)
 
diff --git a/hw/xen/xen_pt_config_init.c b/hw/xen/xen_pt_config_init.c
index dae0519..68b8f22 100644
--- a/hw/xen/xen_pt_config_init.c
+++ b/hw/xen/xen_pt_config_init.c
@@ -1016,13 +1016,9 @@ static XenPTRegInfo xen_pt_emu_reg_pm[] = {
  */
 
 /* Helper */
-static bool xen_pt_msgdata_check_type(uint32_t offset, uint16_t flags)
-{
-    /* check the offset whether matches the type or not */
-    bool is_32 = (offset == PCI_MSI_DATA_32) && !(flags & PCI_MSI_FLAGS_64BIT);
-    bool is_64 = (offset == PCI_MSI_DATA_64) &&  (flags & PCI_MSI_FLAGS_64BIT);
-    return is_32 || is_64;
-}
+#define xen_pt_msi_check_type(offset, flags, what) \
+        ((offset) == ((flags) & PCI_MSI_FLAGS_64BIT ? \
+                      PCI_MSI_##what##_64 : PCI_MSI_##what##_32))
 
 /* Message Control register */
 static int xen_pt_msgctrl_reg_init(XenPCIPassthroughState *s,
@@ -1134,7 +1130,45 @@ static int xen_pt_msgdata_reg_init(XenPCIPassthroughState *s,
     uint32_t offset = reg->offset;
 
     /* check the offset whether matches the type or not */
-    if (xen_pt_msgdata_check_type(offset, flags)) {
+    if (xen_pt_msi_check_type(offset, flags, DATA)) {
+        *data = reg->init_val;
+    } else {
+        *data = XEN_PT_INVALID_REG;
+    }
+    return 0;
+}
+
+/* this function will be called twice (for 32 bit and 64 bit type) */
+/* initialize Mask register */
+static int xen_pt_mask_reg_init(XenPCIPassthroughState *s,
+                                XenPTRegInfo *reg, uint32_t real_offset,
+                                uint32_t *data)
+{
+    uint32_t flags = s->msi->flags;
+
+    /* check the offset whether matches the type or not */
+    if (!(flags & PCI_MSI_FLAGS_MASKBIT)) {
+        *data = XEN_PT_INVALID_REG;
+    } else if (xen_pt_msi_check_type(reg->offset, flags, MASK)) {
+        *data = reg->init_val;
+    } else {
+        *data = XEN_PT_INVALID_REG;
+    }
+    return 0;
+}
+
+/* this function will be called twice (for 32 bit and 64 bit type) */
+/* initialize Pending register */
+static int xen_pt_pending_reg_init(XenPCIPassthroughState *s,
+                                   XenPTRegInfo *reg, uint32_t real_offset,
+                                   uint32_t *data)
+{
+    uint32_t flags = s->msi->flags;
+
+    /* check the offset whether matches the type or not */
+    if (!(flags & PCI_MSI_FLAGS_MASKBIT)) {
+        *data = XEN_PT_INVALID_REG;
+    } else if (xen_pt_msi_check_type(reg->offset, flags, PENDING)) {
         *data = reg->init_val;
     } else {
         *data = XEN_PT_INVALID_REG;
@@ -1222,7 +1256,7 @@ static int xen_pt_msgdata_reg_write(XenPCIPassthroughState *s,
     uint32_t offset = reg->offset;
 
     /* check the offset whether matches the type or not */
-    if (!xen_pt_msgdata_check_type(offset, msi->flags)) {
+    if (!xen_pt_msi_check_type(offset, msi->flags, DATA)) {
         /* exit I/O emulator */
         XEN_PT_ERR(&s->dev, "the offset does not match the 32/64 bit type!\n");
         return -1;
@@ -1267,7 +1301,7 @@ static XenPTRegInfo xen_pt_emu_reg_msi[] = {
         .size       = 2,
         .init_val   = 0x0000,
         .ro_mask    = 0xFF8E,
-        .emu_mask   = 0x007F,
+        .emu_mask   = 0x017F,
         .init       = xen_pt_msgctrl_reg_init,
         .u.w.read   = xen_pt_word_reg_read,
         .u.w.write  = xen_pt_msgctrl_reg_write,
@@ -1316,6 +1350,50 @@ static XenPTRegInfo xen_pt_emu_reg_msi[] = {
         .u.w.read   = xen_pt_word_reg_read,
         .u.w.write  = xen_pt_msgdata_reg_write,
     },
+    /* Mask reg (if PCI_MSI_FLAGS_MASKBIT set, for 32-bit devices) */
+    {
+        .offset     = PCI_MSI_MASK_32,
+        .size       = 4,
+        .init_val   = 0x00000000,
+        .ro_mask    = 0xFFFFFFFF,
+        .emu_mask   = 0xFFFFFFFF,
+        .init       = xen_pt_mask_reg_init,
+        .u.dw.read  = xen_pt_long_reg_read,
+        .u.dw.write = xen_pt_long_reg_write,
+    },
+    /* Mask reg (if PCI_MSI_FLAGS_MASKBIT set, for 64-bit devices) */
+    {
+        .offset     = PCI_MSI_MASK_64,
+        .size       = 4,
+        .init_val   = 0x00000000,
+        .ro_mask    = 0xFFFFFFFF,
+        .emu_mask   = 0xFFFFFFFF,
+        .init       = xen_pt_mask_reg_init,
+        .u.dw.read  = xen_pt_long_reg_read,
+        .u.dw.write = xen_pt_long_reg_write,
+    },
+    /* Pending reg (if PCI_MSI_FLAGS_MASKBIT set, for 32-bit devices) */
+    {
+        .offset     = PCI_MSI_MASK_32 + 4,
+        .size       = 4,
+        .init_val   = 0x00000000,
+        .ro_mask    = 0xFFFFFFFF,
+        .emu_mask   = 0x00000000,
+        .init       = xen_pt_pending_reg_init,
+        .u.dw.read  = xen_pt_long_reg_read,
+        .u.dw.write = xen_pt_long_reg_write,
+    },
+    /* Pending reg (if PCI_MSI_FLAGS_MASKBIT set, for 64-bit devices) */
+    {
+        .offset     = PCI_MSI_MASK_64 + 4,
+        .size       = 4,
+        .init_val   = 0x00000000,
+        .ro_mask    = 0xFFFFFFFF,
+        .emu_mask   = 0x00000000,
+        .init       = xen_pt_pending_reg_init,
+        .u.dw.read  = xen_pt_long_reg_read,
+        .u.dw.write = xen_pt_long_reg_write,
+    },
     {
         .size = 0,
     },
diff --git a/include/hw/pci/pci_regs.h b/include/hw/pci/pci_regs.h
index 56a404b..57e8c80 100644
--- a/include/hw/pci/pci_regs.h
+++ b/include/hw/pci/pci_regs.h
@@ -298,8 +298,10 @@
 #define PCI_MSI_ADDRESS_HI	8	/* Upper 32 bits (if PCI_MSI_FLAGS_64BIT set) */
 #define PCI_MSI_DATA_32		8	/* 16 bits of data for 32-bit devices */
 #define PCI_MSI_MASK_32		12	/* Mask bits register for 32-bit devices */
+#define PCI_MSI_PENDING_32	16	/* Pending bits register for 32-bit devices */
 #define PCI_MSI_DATA_64		12	/* 16 bits of data for 64-bit devices */
 #define PCI_MSI_MASK_64		16	/* Mask bits register for 64-bit devices */
+#define PCI_MSI_PENDING_64	20	/* Pending bits register for 32-bit devices */
 
 /* MSI-X registers */
 #define PCI_MSIX_FLAGS		2
-- 
2.2.1

